DScaler -- BT8x8 Advanced Settings

| BT8x8 Advanced Settings

Advanced Settings for CX2388x based cards. The default values are chosen to work well with most situations and usually do not need to be changed.

Setting | Default | Description
--- | --- | ---
Horizontal Delay | 0 | Number of half lines to skip at the top before we start capturing. 0 means use default for format.
Vertical Delay | 0 | Period to skip on the left before we start capturing. 0 means use default for format.
Eat Lines at Top | 25 | (H3D Specific) Discards lines at the top of the SDI input when in non-progressive mode.