DScaler -- Timing Settings

| Timing Settings

Settings specific to flip timing

Setting | Default | Description
--- | --- | ---
Auto Format Detect | ON | Should we try and spot input format changes
50Hz Format | PAL | Mode to use when 50Hz input is detected
60Hz Format | NTSC | Mode to use when 60Hz input is detected
Format Change Threshold | 2 | Number of ten field periods when the timing pattern must be repeated before switching.
Do JudderTerminator On Video Modes | OFF | If global JudderTerminator is on then should it be used in video mode.
Sleep Interval | 0 | Number of ms to sleep when waiting.
Sleep Skip Fields | 0 | Can be used to only sleep every so many frames.
Sleep Skip Fields Late | 0 | Can be used to only sleep every so many frames when running late.