DScaler -- MoComp2

| MoComp2

This is a new method that should be considered a work in progress. At the moment it is a motion adaptive method with diagonal interpolation based on:

T. Chen, H.R. Wu; & Z.H. Yu,
"Efficient deinterlacing algorithm using edge-based line average interpolation"
Optical Engineering, Volume 39, Issue 8, (2000)

This method also incorporates built in chroma smoothing to help disguise MPEG chroma problems.

Who Should Use It?

The method should be a general use one but at the moment most consider TomsMoComp to give a better picture. As this method uses less CPU than TomsMoComp it may be well suited to those who run a lot of filters. Note the built in chroma smoother means that this method may give better results with digital sourced material such as DVD or DVB.

The Settings

There are currently no user settings. The search effort setting currently has no effect.